**Mineral Exploration Reporting Templates**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Template Name** | **Template** | **Example Template with Instructions - File Name** | **Example Blank Template - File Name** | **Data Type** |
| Surface Location - Mapping | SL4 | GSV\_VICSL4\_MAPPING\_Example.xlsx | GSV\_VICSL4\_MAPPING\_Blank\_Example.xlsx | Surface point locations: mapping point data (leave drilling information fields blank) |
| Geochemical Sampling - Laboratory | SG4 | GSV\_VICSG4\_S-GEOCHEM\_Example.xlsx | GSV\_VICSG4\_S-GEOCHEM\_Blank\_Example.xlsx | Geochemical sampling data - Laboratory |
| Geochemical Sampling – Portable XRF | SG4\_PXRF | GSV\_VICSG4\_S-GEOCHEM-PXRF\_Example.xlsx | GSV\_VICSG4\_S-GEOCHEM-PXRF\_Blank\_Example.xlsx | Geochemical sampling data - Portable XRF |
| Geochemical Sampling Quality Control - Laboratory | SQG4 | GSV\_VICSQG4\_S-QAQC\_Example.xlsx | GSV\_VICSQG4\_S-QAQC\_Blank\_Example.xlsx | QA/QC data for geochemical sampling - Laboratory: standards, blanks, field duplicates |
| Geochemical Sampling Quality Control – Portable XRF | SQG4\_PXRF | GSV\_VICSQG4\_S-QAQC-PXRF\_Example.xlsx | GSV\_VICSQG4\_S-QAQC-PXRF\_Blank\_Example.xlsx | QA/QC data for geochemical sampling - Portable XRF: standards, blanks, field duplicates |
| Drillhole Location - Collar (Mandatory for all drilling) | SL4 | GSV\_VICSL4\_DH-COLLAR\_Example.xlsx | GSV\_VICSL4\_DH-COLLAR\_Blank\_Example.xlsx | Drill collar data |
| Downhole Survey  (Mandatory for all drilling) | DS4 | GSV\_VICDS4\_DH-SURVEY\_Example.xlsx | GSV\_VICDS4\_DH-SURVEY\_Blank\_Example.xlsx | Downhole directional survey data |
| Downhole Logging (referred to in Australian requirements as downhole lithology) | DL4 | GSV\_VICDL4\_DH-GEO\_Example.xlsx | GSV\_VICDL4\_DH-GEO\_Blank\_Example.xlsx | Downhole logs. All geological, petrophysical and geophysical downhole data. Multiple DL4 files can be provided |
| Downhole Geochemistry - Laboratory | DG4 | GSV\_VICDG4\_DH-GEOCHEM\_Example.xlsx | GSV\_VICDG4\_DH-GEOCHEM\_Blank\_Example.xlsx | Downhole geochemical data - Laboratory |
| Downhole Geochemistry – Portable XRF | DG4\_PXRF | GSV\_VICDG4\_DH-GEOCHEM-PXRF\_Example.xlsx | GSV\_VICDG4\_DH-GEOCHEM-PXRF\_Blank\_Example.xlsx | Downhole geochemical data - portable XRF |
| Downhole Geochemistry Quality Control – Laboratory | DQG4 | GSV\_VICDQG4\_DH-QAQC\_Example.xlsx | GSV\_VICDQG4\_DH-QAQC\_Blank\_Example.xlsx | Drilling QA/QC data - Laboratory: geochemical standards, blanks, field duplicates |
| Downhole Geochemistry Quality Control – Portable XRF | DQG4\_PXRF | GSV\_VICDQG4\_DH-QAQC-PXRF\_Example.xlsx | GSV\_VICDQG4\_DH-QAQC-PXRF\_Blank\_Example.xlsx | Drilling QA/QC data - Portable XRF: geochemical standards, blanks, field duplicates |